(footprint "CP_Radial_D8.0mm_P3.50mm_horizontal" (version 20211014) (generator pcbnew)
  (layer "F.Cu")
  (tedit 5AE50EF0)
  (descr "CP, Radial series, Radial, pin pitch=3.50mm, , diameter=8mm, Electrolytic Capacitor")
  (tags "CP Radial series Radial pin pitch 3.50mm  diameter 8mm Electrolytic Capacitor")
  (attr through_hole)
  (fp_text reference "REF**" (at 1.75 -5.25) (layer "F.SilkS")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp dfe7c6f4-3d35-4c8d-92d0-7da79e80ded9)
  )
  (fp_text value "CP_Radial_D8.0mm_P3.50mm" (at 1.75 5.25) (layer "F.Fab")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 46f3fdce-2486-4415-91d2-94e33bdeb753)
  )
  (fp_text user "${REFERENCE}" (at 1.75 0) (layer "F.Fab")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 19cde737-6f64-4a4e-bbc6-a70404d9f27e)
  )
  (fp_line (start -1.65 1.6) (end -1.65 2.4) (layer "F.SilkS") (width 0.12) (tstamp 4b9cbc51-7b5a-4691-b115-0e3235035551))
  (fp_line (start 1.75 0) (end -2.25 0) (layer "F.SilkS") (width 0.12) (tstamp 52ef12f1-3cad-45fe-a009-289d4b8ed21c))
  (fp_line (start 4.8 5.5) (end 5.6 5.5) (layer "F.SilkS") (width 0.12) (tstamp 769b7bea-e66d-46de-b1b6-bd86097e7786))
  (fp_line (start -2.05 2) (end -1.25 2) (layer "F.SilkS") (width 0.12) (tstamp b14faded-ebee-4ef4-8f83-876f8677fcd2))
  (fp_line (start 0 0) (end 1.75 0) (layer "F.SilkS") (width 0.12) (tstamp b35d7071-d584-4ccb-a3c2-48a55ac1a157))
  (fp_rect (start -2.25 0) (end 5.75 -20) (layer "F.SilkS") (width 0.15) (fill none) (tstamp 09e5ccf2-b717-4754-8145-2e8bdc7c80dd))
  (fp_rect (start 3.4 4.5) (end 3.6 0) (layer "F.SilkS") (width 0.12) (fill solid) (tstamp 21189435-5696-49f1-bc84-fed0bd89c3a7))
  (fp_rect (start -0.1 1) (end 0.1 0) (layer "F.SilkS") (width 0.12) (fill solid) (tstamp 9a38bb25-f64e-4664-b022-7ac6783469fe))
  (fp_rect (start -2.35 0.1) (end 5.85 -20.1) (layer "F.CrtYd") (width 0.05) (fill none) (tstamp 607810e5-63cd-40b7-8d58-b229305ea84b))
  (fp_line (start -1.676759 -1.7475) (end -0.876759 -1.7475) (layer "F.Fab") (width 0.1) (tstamp 0deaf689-a9b8-44d7-8597-97672a70b331))
  (fp_line (start -1.276759 -2.1475) (end -1.276759 -1.3475) (layer "F.Fab") (width 0.1) (tstamp e010dbf8-2557-4475-b757-556d79952a45))
  (fp_rect (start -2.15 -0.1) (end 5.65 -19.9) (layer "F.Fab") (width 0.05) (fill none) (tstamp 210fb83e-ece9-4d71-b271-9ef03a01a380))
  (pad "1" thru_hole rect (at 0 2) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask) (tstamp 71eb0b98-d495-454c-aa36-62aa5b70781f))
  (pad "2" thru_hole circle (at 3.5 5.5) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask) (tstamp c605e50c-0020-44b7-9271-6776795f5350))
  (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/CP_Radial_D8.0mm_P3.50mm.wrl"
    (offset (xyz 0 0 4))
    (scale (xyz 1 1 2.5))
    (rotate (xyz 90 0 0))
  )
)
