# NeoPixelBus

[![Donate](https://img.shields.io/badge/paypal-donate-yellow.svg)](https://www.paypal.com/cgi-bin/webscr?cmd=_s-xclick&hosted_button_id=6AA97KE54UJR4)

Arduino NeoPixel library

A library to control one wire protocol RGB, RGBW, and RGBWW leds like APA106, SK6812, WS2811, WS2812 and WS2813 that are commonly refered to as NeoPixels and two wire protocol RGB like Lpd8806, APA102 and SK9822 commonly refered to as DotStars.
Supports most Arduino platforms.  

For quick questions and support:  
* [Try the new Github Discussions](https://github.com/Makuna/NeoPixelBus/discussions)  
* [Discord NeoPixelBus Invitation](https://discord.gg/c6FrysvZyV) or if you are already a member of [Discord Server NeoPixelBus](https://discord.com/channels/789177382221119519/789177382221119521)  
* Or jump on Gitter   
[![Gitter](https://badges.gitter.im/Join%20Chat.svg)](https://gitter.im/Makuna/NeoPixelBus?utm_source=badge&utm_medium=badge&utm_campaign=pr-badge)  

For bugs, make sure there isn't an active issue and then create one.

## Documentation
[See Wiki](https://github.com/Makuna/NeoPixelBus/wiki)

## Installing This Library (preferred, you just want to use it)
Open the Library Manager and search for "NeoPixelBus by Makuna" and install

## Installing This Library From GitHub (advanced, you want to contribute)
Create a directory in your Arduino\Library folder named "NeoPixelBus"
Clone (Git) this project into that folder.  
It should now show up in the import list when you restart Arduino IDE.





