# PIXELIX <!-- omit in toc -->
![PIXELIX](../../../images/LogoBlack.png)

[![License](https://img.shields.io/badge/license-MIT-blue.svg)](http://choosealicense.com/licenses/mit/)

# BOM <!-- omit in toc -->

- [List](#list)
- [Issues, Ideas And Bugs](#issues-ideas-and-bugs)
- [License](#license)
- [Contribution](#contribution)

# List

| Amount | Description | Package | Part | URL |
| --- | --- | --- | --- | --- |
| 2 | Capacitor 10 pF | C1206 | C3, C4 | [Reichelt](https://www.reichelt.de/smd-vielschicht-keramikkondensator-10p-5-npo-g1206-10p-p31885.html?&trstct=pol_2) |
| 3 | Capacitor 100 nF | C1206 | C1, C5, C6 | [Reichelt](https://www.reichelt.de/vielschicht-kerko-100nf-50v-125-c-kem-x7r1206b100n-p207152.html?) |
| 1 | Capacitor 1000 uF / 16 V | E5-8.5 | C2 | [Reichelt](https://www.reichelt.de/elko-radial-1-0-mf-16-v-105-c-low-esr-rad-fr-1-000-16-p121253.html?) |
| 4 | Resistor 100 Ohm | R1206 | R6, R7, R8, R9 | [Reichelt](https://www.reichelt.de/smd-widerstand-1206-100-ohm-250-mw-5-smd-1-4w-100-p18242.html?r=1) |
| 1 | Resistor 1 kOhm | R1206 | R4 | [Reichelt](https://www.reichelt.de/smd-widerstand-1206-1-0-kohm-250-mw-5-smd-1-4w-1-0k-p18221.html?r=1)  |
| 1 | Resistor 1.2 kOhm | R1206 | R2 | [Reichelt](https://www.reichelt.de/smd-widerstand-1206-1-2-kohm-250-mw-5-smd-1-4w-1-2k-p18227.html?r=1)  |
| 1 | Resistor 10 kOhm | R1206 | R3 | [Reichelt](https://www.reichelt.de/smd-widerstand-1206-10-kohm-250-mw-5-smd-1-4w-10k-p18244.html?r=1) |
| 1 | Resistor 100 kOhm | R1206 | R1 | [Reichelt](https://www.reichelt.de/smd-widerstand-1206-100-kohm-250-mw-1-koa-rk73h2bttd14-p238058.html?) |
| 1 | Resistor 8.2 MOhm | R1206 | R5 | [Reichelt](https://www.reichelt.de/smd-widerstand-1206-8-2-mohm-250-mw-5-smd-1-4w-8-2m-p18377.html?)  |
| 1 | Harting connector | ML10 | CON1 | [Reichelt](https://www.reichelt.de/wannenstecker-10-polig-gerade-wsl-10g-p22816.html?)  |
| 1 | ESD suppressor CDSOD323-T05C | SOD-323 | D1 | [Conrad](https://www.conrad.de/de/p/bourns-tvs-diode-cdsod323-t05c-sod-323-6-v-350-w-1055444.html?searchType=SearchRedirect), [Farnell](https://de.farnell.com/bourns/cdsod323-t05c/tvs-diode-bidir-1-line-5v-sod323/dp/1824860?st=TVS-Diode%20CDSOD323-T05C) |
| 1 | Micro fuse block, 4A slow | OMNI-BLOK | F1 | [Reichelt](https://www.reichelt.de/smd-sicherungshalter-mit-sicherung-4-0-a-125-v-traege-litt-0154004-drt-p229203.html?&trstct=pos_9), [Farnell](https://de.farnell.com/littelfuse/0154004-drt/sicherung-smd-omni-block-t-4a/dp/9943765?st=smd%20OMNI-BLOK) |
| 1 | ESP32-DEVKIT V1 | - | ESP32-DEVKITV1 | [Ebay](https://www.ebay.de/itm/Espressif-ESP32-WLAN-Dev-Kit-Board-Development-Bluetooth-Wifi-v1-WROOM32-NodeMCU/253059783728?ssPageName=STRK%3AMEBIDX%3AIT&_trksid=p2057872.m2749.l2649) |
| 1 | N-channel mosfet BSS138 | SOT23 | Q1 | [Reichelt](https://www.reichelt.de/mosfet-n-ch-50v-0-22a-0-36w-sot-23-bss-138-smd-p41437.html?), [Farnell](https://de.farnell.com/on-semiconductor/bss138/mosfet-n-kanal-50v-220ma-sot-23/dp/9845330?st=N-channel%20mosfet%20BSS138) |
| 1 | 32.768 kHz crystal | TC26V | Q2 | [Reichelt](https://www.reichelt.de/standardquarz-grundton-32-768-khz-iqd-lfxtal014219-p245417.html?), [Farnell](https://de.farnell.com/citizen-finedevice/cfs206-32-768kdzb-ub/quarz-uhr-32-768khz-zylinder-6pf/dp/1457085?st=32.768%20kHz)  |
| 1 | P-channel mosfet STD26P3LLH6 | TO252 | U1 | [Reichelt](https://www.reichelt.de/mosfet-p-ch-30v-12a-0-03r-to252-std26p3llh6-p254904.html?), [Farnell](https://de.farnell.com/stmicroelectronics/std26p3llh6/mosfet-p-kanal-30v-12a-to-252/dp/2629747?st=STD26P3LLH6) |
| 6 | Wago clamp 2 | W237-102 | X1, X2, X3, X4, X5, X6 | [Reichelt](https://www.reichelt.de/thr-leiterplattenklemme-rm-4-mm-2-pol-sw-wago-2060-1422-p163238.html?), [Farnell](https://de.farnell.com/wago/2060-472-998-404/reihenklemme-wire-to-board-2pos/dp/2916184?st=WAGO%202060-1422) |
| 1 | Wago clamp 1 | W237-103 | X2 | [Reichelt](https://www.reichelt.de/thr-leiterplattenklemme-rm-4-mm-1-pol-sw-wago-2060-1421-p163237.html?&trstct=lsbght_sldr::163234) |
| 1 | WS2812B 5050 8x32 RGB Flexible LED Panel Matrix | - | - | [Ebay](https://www.ebay.de/itm/WS2812B-5050-8x32-RGB-Flexible-LED-Panel-Matrix-Programmable-Display-Screen-DE/223166536588?ssPageName=STRK%3AMEBIDX%3AIT&_trksid=p2057872.m2749.l2649) |
| 1 | Power supply 5 V / 5 A (4 A would be enough) | - | - | [Reichelt](https://www.reichelt.de/tischnetzteil-25-w-5-v-5-a-mw-gst40a05-p171043.html?&trstct=pol_1) |
| 1 | Power cable | - | - | [Reichelt](https://www.reichelt.de/netzkabel-schutzkontaktstecker-gew-1-8-m-schw-c13-nksk-200-sw-p13490.html?r=1) |
| 1 | Power supply plug | - | - | [Reichelt](https://www.reichelt.de/einbaukupplung-fuer-hohlstecker-aussen-5-6mm-innen-2-1mm-lum-1614-19-p237595.html?&trstct=pol_0) |

Note, X2 is a composition of Wago clamp 1 and 2.

# Issues, Ideas And Bugs
If you have further ideas or you found some bugs, great! Create a [issue](https://github.com/BlueAndi/esp-rgb-led-matrix/issues) or if you are able and willing to fix it by yourself, clone the repository and create a pull request.

# License
The whole source code is published under the [MIT license](http://choosealicense.com/licenses/mit/).
Consider the different licenses of the used third party libraries too!

# Contribution
Unless you explicitly state otherwise, any contribution intentionally submitted for inclusion in the work by you, shall be licensed as above, without any
additional terms or conditions.
