# PIXELIX
![PIXELIX](../../../images/LogoBlack.png)

[![License](https://img.shields.io/badge/license-MIT-blue.svg)](http://choosealicense.com/licenses/mit/)

# BOM

| Amount | Description | Package | Part | URL |
| --- | --- | --- | --- | --- |
| 1 | Adafruit Feather V2 | Feather V2 | A1 | [Adafruit](https://www.adafruit.com/product/5400), [Amazon](https://www.amazon.de/-/en/Adafruit-ESP32-Feather-V2-8MB-Flash/dp/B0BB2WF9HV/), [Mouser](https://www.mouser.de/ProductDetail/Adafruit/5400?qs=MyNHzdoqoQJczdKY45yRtg%3D%3D) |
| 3 | Capacitor 100 nF | C1206 | C1, C3, C4 | [Reichelt](https://www.reichelt.de/vielschicht-kerko-100nf-50v-125-c-kem-x7r1206b100n-p207152.html?), [Mouser](https://www.mouser.de/ProductDetail/KEMET/C1206C104K5RACTM?qs=ED%252B2xvMfDz2aaotiiWTrQg%3D%3D) |
| 1 | Capacitor 1000 uF / 16 V | E5-8.5 | C2 | [Reichelt](https://www.reichelt.de/elko-radial-1-0-mf-16-v-105-c-low-esr-rad-fr-1-000-16-p121253.html?), [Mouser](https://www.mouser.de/ProductDetail/Panasonic/EEU-FR1C102L?qs=ATUT3BIXiFhT8tblOBeOAQ%3D%3D) |
| 4 | Resistor 100 Ohm | R1206 | R5, R6, R7, R8 | [Reichelt](https://www.reichelt.de/smd-widerstand-1206-100-ohm-250-mw-5-smd-1-4w-100-p18242.html?r=1), [Mouser](https://www.mouser.de/ProductDetail/YAGEO/RC1206JR-07100RL?qs=afJZr%2F7kGG7feudZTJCmlw%3D%3D) |
| 1 | Resistor 1 kOhm | R1206 | R2 | [Reichelt](https://www.reichelt.de/smd-widerstand-1206-1-0-kohm-250-mw-5-smd-1-4w-1-0k-p18221.html?r=1), [Mouser](https://www.mouser.de/ProductDetail/YAGEO/RC1206JR-071KL?qs=CteSnpDdeuB6ARqGTIgKSQ%3D%3D)  |
| 1 | Resistor 1.2 kOhm | R1206 | R3 | [Reichelt](https://www.reichelt.de/smd-widerstand-1206-1-2-kohm-250-mw-5-smd-1-4w-1-2k-p18227.html?r=1), [Mouser](https://www.mouser.de/ProductDetail/YAGEO/RC1206JR-071K2L?qs=CteSnpDdeuDgiTTZVtL9%2FQ%3D%3D)  |
| 1 | Resistor 10 kOhm | R1206 | R1 | [Reichelt](https://www.reichelt.de/smd-widerstand-1206-10-kohm-250-mw-5-smd-1-4w-10k-p18244.html?r=1), [Mouser](https://www.mouser.de/ProductDetail/YAGEO/RC1206JR-0710KL?qs=afJZr%2F7kGG7jis1hiCdUVA%3D%3D) |
| 1 | Resistor 100 kOhm | R1206 | R4 | [Reichelt](https://www.reichelt.de/smd-widerstand-1206-100-kohm-250-mw-1-koa-rk73h2bttd14-p238058.html?), [Mouser](https://www.mouser.de/ProductDetail/YAGEO/RC1206FR-07100KL?qs=XiHlnyMtlzIPjdId8aaAEA%3D%3D) |
| 1 | ESD suppressor CDSOD323-T05C | SOD-323 | D1 | [Conrad](https://www.conrad.de/de/p/bourns-tvs-diode-cdsod323-t05c-sod-323-6-v-350-w-1055444.html?searchType=SearchRedirect), [Farnell](https://de.farnell.com/bourns/cdsod323-t05c/tvs-diode-bidir-1-line-5v-sod323/dp/1824860?st=TVS-Diode%20CDSOD323-T05C), [Mouser](https://www.mouser.de/ProductDetail/Bourns/CDSOD323-T05C?qs=N%252BiqXe0%252BQtutiz%2Fj8zPmAQ%3D%3D) |
| 1 | Micro fuse block, 4A slow | OMNI-BLOK | F1 | [Reichelt](https://www.reichelt.de/smd-sicherungshalter-mit-sicherung-4-0-a-125-v-traege-litt-0154004-drt-p229203.html?&trstct=pos_9), [Farnell](https://de.farnell.com/littelfuse/0154004-drt/sicherung-smd-omni-block-t-4a/dp/9943765?st=smd%20OMNI-BLOK), [Mouser](https://www.mouser.de/ProductDetail/?qs=gu7KAQ731UQeedYeniUNnQ%3D%3D) |
| 1 | Espressif ESP32-DEVKIT | ESP32-DEVKITC-32D | U1 | [Mouser](https://www.mouser.de/ProductDetail/Espressif-Systems/ESP32-DevKitC-32D?qs=%252BEew9%252B0nqrDsObWEpDx6YQ%3D%3D), [Amazon](https://www.amazon.de/s?k=ESP32-DEVKITC-32D&i=computers&__mk_de_DE=%C3%85M%C3%85%C5%BD%C3%95%C3%91&crid=1JR244SPWCCAG&sprefix=esp32-devkitc-32d+%2Ccomputers%2C99&ref=nb_sb_noss) |
| 1 | N-channel mosfet BSS138 | SOT23 | Q1 | [Reichelt](https://www.reichelt.de/mosfet-n-ch-50v-0-22a-0-36w-sot-23-bss-138-smd-p41437.html?), [Farnell](https://de.farnell.com/on-semiconductor/bss138/mosfet-n-kanal-50v-220ma-sot-23/dp/9845330?st=N-channel%20mosfet%20BSS138), [Mouser](https://www.mouser.de/ProductDetail/onsemi-Fairchild/BSS138?qs=HK%252BeIG1iaahCeqBvjB4arg%3D%3D) |
| 1 | P-channel mosfet STD26P3LLH6 | TO252 | Q2 | [Reichelt](https://www.reichelt.de/mosfet-p-ch-30v-12a-0-03r-to252-std26p3llh6-p254904.html?), [Farnell](https://de.farnell.com/stmicroelectronics/std26p3llh6/mosfet-p-kanal-30v-12a-to-252/dp/2629747?st=STD26P3LLH6), [Mouser](https://www.mouser.de/ProductDetail/STMicroelectronics/STD26P3LLH6?qs=DqCdCwOw4%2F7LRzP66tTiGg%3D%3D) |
| 5 | Conn_01x02 | Wuerth Elektronik 66200211022 | J1, J2, J4, J6, J8 | [Farnell](https://de.farnell.com/wurth-elektronik/66200211022/steckv-stiftleiste-2pos-1reihe/dp/2827850?ost=66200211022), [Mouser](https://www.mouser.de/c/?q=66200211022) |
| 2 | Conn_01x03 | Wuerth Elektronik 66200311022 | J3, J7 | [Farnell](https://de.farnell.com/wurth-elektronik/66200311022/stiftleiste-abgew-3pos-1-reihe/dp/3818193?ost=66200311022), [Mouser](https://www.mouser.de/ProductDetail/Wurth-Elektronik/66200311022?qs=3RJ0PdSuLVkSi7ZZT4Z8xA%3D%3D) |
| 1 | Conn_02x05_Odd_Even | Wuerth Elektronik 61201021621 | J5 | [Farnell](https://de.farnell.com/wurth-elektronik/61201021621/stiftleiste-2-54mm-gerade-10pol/dp/1642019?ost=61201021621), [Mouser](https://www.mouser.de/ProductDetail/Wurth-Elektronik/61201021621?qs=W%252B2sBeLta1a0dwX5pxbfXw%3D%3D) |
| --- | --- | --- | --- | --- |
| 5 | Plug_01x02 | Wuerth Elektronik 662002013322 | J1*, J2*, J4*, J6*, J8* | [Mouser](https://www.mouser.de/ProductDetail/Wurth-Elektronik/662002013322?qs=2kOmHSv6VfRYc3%2FxPP%2FegA%3D%3D) |
| 2 | Plug_01x03 | Wuerth Elektronik 662003013322 | J3*, J7* | [Mouser](https://www.mouser.de/ProductDetail/Wurth-Elektronik/662003013322?qs=E2PpAYvlWVvj7tqTtujsuA%3D%3D) |
| 1 | WS2812B 5050 8x32 RGB Flexible LED Panel Matrix | - | - | [Amazon](https://www.amazon.de/CHINLY-Flexible-Individuellement-adressable-%C3%A9clairage/dp/B07418XNJ2/) |
| 1 | Power supply 5 V / 5 A (4 A would be enough) | - | - | [Reichelt](https://www.reichelt.de/tischnetzteil-25-w-5-v-5-a-mw-gst40a05-p171043.html?&trstct=pol_1), [Mouser](https://www.mouser.de/ProductDetail/CUI-Inc/SDM36-5-U-P5?qs=sGAEpiMZZMvasLKgtn5bIdlT96xMCNovx7vHF9wwR4Ri0p1WQs8y5w%3D%3D) |
| 1 | Power cable | - | - | [Reichelt](https://www.reichelt.de/netzkabel-schutzkontaktstecker-gew-1-8-m-schw-c13-nksk-200-sw-p13490.html?r=1), [Mouser](https://www.mouser.de/ProductDetail/Qualtek/364002-D01?qs=HFfMDpzxxd3ZLZg3BXSDag%3D%3D) |
| 1 | Power supply plug | - | - | [Mouser](https://www.mouser.de/ProductDetail/CUI-Devices/PJ-065A?qs=WyjlAZoYn53baW2eG%252Bovnw%3D%3D) |
| 1 | USER-Button | - | - | [Amazon](https://www.amazon.de/-/en/gp/product/B08L49F7DV) |
| 1 | RESET-Button | - | - | [Amazon](https://www.amazon.de/-/en/gp/product/B08YMZGLWX) |
| 1 | Light Sensor  | LDR5528  | - | [Amazon](https://www.amazon.de/-/en/AZDelivery-pieces-resistor-diodes-LDR5528/dp/B089YNCYG4) |
| 1 | Audio Sensor-Module | INMP441  | - | [Amazon](https://www.amazon.de/-/en/gp/product/B09JFDJ9BF) |
| 4 | Insert-Nuts M2 | - | - | [Amazon](https://www.amazon.de/ruthex-Gewindeeinsatz-St%C3%BCck-Gewindebuchsen-Kunststoffteile/dp/B088QJG676/)

* Note, only **ONE** ESP32 is required. Either U1 or A1.
* Note, you can also use the *Molex 2157601002* connectors for J1, J2, J4, J6 and J8 and the *Molex 2157601003* for J3 and J7.
* Note, you can also use the *Molex 2157591002* plugs for J1*, J2*, J4*, J6* and J8* and the *Molex 2157591003* for J3* and J7*. You also need crimp terminals (e.g. *Wuerth Elektronik 66200113722DEC* or *Molex 2064600021*)
* Do **NOT** combine connectors and plugs from Molex and Wuerth Elektronik!

# Issues, Ideas And Bugs
If you have further ideas or you found some bugs, great! Create a [issue](https://github.com/BlueAndi/esp-rgb-led-matrix/issues) or if you are able and willing to fix it by yourself, clone the repository and create a pull request.

# License
The whole source code is published under the [MIT license](http://choosealicense.com/licenses/mit/).
