# DDPPlugin

The plugin setup a server supporting the Distributed Display Protocol (DDP), which is used e.g. by xlights or LedFx.

Supported formats:

- RGB with 24-bit per pixel

## xlights Configuration

### Add Ethernet controller

- Name: Pixelix
- IP Address:<IP-ADDRESS>
- Protocol: DDP

### Add Layout

#### Create new matrix

- Name: Matrix8x32

#### Matrix

- Direction: Horizontal
- Strings: 8
- Nodes/String: 32
- Strands/String: 1
- Starting Location: Top Left
- Controller: Pixelix

#### Controller Connection

- Port: 1
- Protocol: LED Panel Matrix

#### String Properties

- String Type: RGB Nodes

#### Appearance

- Pixel Size: 10
- Pixel Style: Square

## REST API

    -